;****************************************************************************************
;
; rt2500usb.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   Ralink RT2500 series USB Wireless LAN Card.
;
;   Copyright (c)2004, Ralink Technology Corp., All Rights Reserved
;   All Rights Reserved.
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Provider%
Compatible      = 1
DriverVer       = 07/15/2004, 1.02.00.0000
CatalogFile    = rt2500usb.CAT            ;for WHQL certified

[ControlFlags]
;***********Ralink 802.11g board  ***********
;ExcludeFromSelect = USB\VID_148F&PID_2570

[Manufacturer]
%Ralink%        = Ralink
%Amigo%         = Amigo
%MSI%           = MSI
%SMC%           = SMC

[Ralink]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Ralink.DeviceDesc% =       RALINK.ndi,             USB\VID_148F&PID_2570

[Amigo]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Amigo.DeviceDesc%         = AMIGO.ndi,             USB\VID_0EB0&PID_9020

[MSI]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%m2500usb_6861.DeviceDesc% = m2500usb_6861.ndi,     USB\VID_0DB0&PID_6861
%m2500usb_6865.DeviceDesc% = m2500usb_6865.ndi,     USB\VID_0DB0&PID_6865
%m2500usb_6869.DeviceDesc% = m2500usb_6869.ndi,     USB\VID_0DB0&PID_6869

[SMC]
; DisplayName              Section                  DeviceID
; -----------              -------                  --------
%SMC.DeviceDesc%           = SMC.ndi,               USB\VID_0707&PID_EE13

;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[RALINK.ndi]
AddReg                  = Common.reg, RALINK.ndi.reg
CopyFiles               = win9x.CopyFiles

[AMIGO.ndi]
AddReg                  = Common.reg, AMIGO.ndi.reg
CopyFiles               = win9x.CopyFiles

[m2500usb_6861.ndi]
AddReg                  = Common.reg, m2500usb_6861.ndi.reg
CopyFiles               = win9x.CopyFiles

[m2500usb_6865.ndi]
AddReg                  = Common.reg, m2500usb_6865.ndi.reg
CopyFiles               = win9x.CopyFiles

[m2500usb_6869.ndi]
AddReg                  = Common.reg, m2500usb_6869.ndi.reg
CopyFiles               = win9x.CopyFiles

[SMC.ndi]
AddReg                  = Common.reg, SMC.ndi.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[RALINK.ndi.NT]
AddReg                  = Common.reg, RALINK.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[AMIGO.ndi.NT]
AddReg                  = Common.reg, AMIGO.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[m2500usb_6861.ndi.NT]
AddReg                  = Common.reg, m2500usb_6861.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[m2500usb_6865.ndi.NT]
AddReg                  = Common.reg, m2500usb_6865.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[m2500usb_6869.ndi.NT]
AddReg                  = Common.reg, m2500usb_6869.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[SMC.ndi.NT]
AddReg                  = Common.reg, SMC.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

; NT services sections
[RALINK.ndi.NT.Services]
AddService              = RT2500USB, 2, RALINK.Service, common.EventLog

[AMIGO.ndi.NT.Services]
AddService              = RT2500USB, 2, AMIGO.Service, common.EventLog

[m2500usb_6861.ndi.NT.Services]
AddService              = RT2500USB, 2, m2500usb_6861.Service, common.EventLog

[m2500usb_6865.ndi.NT.Services]
AddService              = RT2500USB, 2, m2500usb_6865.Service, common.EventLog

[m2500usb_6869.ndi.NT.Services]
AddService              = RT2500USB, 2, m2500usb_6869.Service, common.EventLog

[SMC.ndi.NT.Services]
AddService              = RT2500USB, 2, SMC.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************


[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,                  0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;
; Select Config Utility
;
HKR, ,                                  ConfigSelect,       0, "0"   ;0=RaConfig, 1=ZeroConfig

;
; Country Region 
;
HKR, ,                                  CountryRegion,      0, "0"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region"
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, "0"
;HKR, NDI\params\CountryRegion\enum,    0,                  0, "FCC (Channel 1 - 11)"
;HKR, NDI\params\CountryRegion\enum,    1,                  0, "IC (Channel 1 - 11)"
;HKR, NDI\params\CountryRegion\enum,    2,                  0, "ETSI (Channel 1 - 13)"
;HKR, NDI\params\CountryRegion\enum,    3,                  0, "Spain (Channel 10 - 11)"
;HKR, NDI\params\CountryRegion\enum,    4,                  0, "France (Channel 10 - 13)"
;HKR, NDI\params\CountryRegion\enum,    5,                  0, "MKK (Channel 14)"
;HKR, NDI\params\CountryRegion\enum,    6,                  0, "MKK1 (Channel 1 - 14)"
;HKR, NDI\params\CountryRegion\enum,    7,                  0, "Israel (Channel 3 - 9)"

;*******************************************************************************************
; Advance Page

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "0"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "0"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "0"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
HKR, ,                            SSID,            0, %SSID_DEF_STR%
HKR, Default,                     SSID,            0, %SSID_DEF_STR%
HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
HKR, NDI\params\SSID,             type,            0, "edit"
HKR, NDI\params\SSID,             limitText,       0, "32"
HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"
HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam,       type,            0, "enum"
HKR, NDI\params\ACPowerCam,       default,         0, "0"
HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "32"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "32"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""


;*******************************************************************************************
; APConfig use
;

;
; WPA Group-Key ReKey Interval
;
HKR, ,                RekeyInterval,   0, "60"

;
; WPA Group-Key ReKey Method
;
HKR, ,                RekeyMethod,     0, "0"


[RALINK.ndi.reg]
HKR, ,                            NTMPDriver,       0, rt25u98.sys
HKR, Ndi,                         DeviceID,         0, "USB\VID_148F&PID_2570"

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "rt25u98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "rt25u98"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;
; Interfaces
;
;
; Install sections
;HKR,Ndi\Install,ndis3,,"rt25u98.install"

[AMIGO.ndi.reg]
HKR, ,                            NTMPDriver,       0, rt25u98.sys
HKR, Ndi,                         DeviceID,         0, "USB\VID_0EB0&PID_9020"

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "rt25u98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "rt25u98"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

[m2500usb_6861.ndi.reg]
HKR, ,                            NTMPDriver,       0, rt25u98.sys
HKR, Ndi,                         DeviceID,         0, "USB\VID_0DB0&PID_6861"

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "rt25u98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "rt25u98"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

[m2500usb_6865.ndi.reg]
HKR, ,                            NTMPDriver,       0, rt25u98.sys
HKR, Ndi,                         DeviceID,         0, "USB\VID_0DB0&PID_6865"

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "rt25u98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "rt25u98"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

[m2500usb_6869.ndi.reg]
HKR, ,                            NTMPDriver,       0, rt25u98.sys
HKR, Ndi,                         DeviceID,         0, "USB\VID_0DB0&PID_6869"

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "rt25u98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "rt25u98"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

[SMC.ndi.reg]
HKR, ,                            NTMPDriver,       0, rt25u98.sys
HKR, Ndi,                         DeviceID,         0, "USB\VID_0707&PID_EE13"

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "rt25u98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "rt25u98"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
win9x.CopyFiles         = 11    ; system32 subdirectory on win9x

[NT.CopyFiles]
rt2500usb.sys                   ; NT Installation

[win9x.CopyFiles]
rt25u98.sys                     ; Win9x Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt2500usb.sys           = 1
rt25u98.sys             = 1


;*******************************************************************************************
; NT specific
;*******************************************************************************************
[Ralink.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt2500usb"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[Ralink.Service]
DisplayName                 = %Ralink.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[AMIGO.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt2500usb"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[AMIGO.Service]
DisplayName                 = %AMIGO.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[m2500usb_6861.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt2500usb"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[m2500usb_6861.Service]
DisplayName                 = %m2500usb.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[m2500usb_6865.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt2500usb"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[m2500usb_6865.Service]
DisplayName                 = %m2500usb.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[m2500usb_6869.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt2500usb"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[m2500usb_6869.Service]
DisplayName                 = %m2500usb.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[SMC.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt2500usb"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[SMC.Service]
DisplayName                = %SMC.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS


[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt2500usb.sys"
HKR, , TypesSupported,   0x00010001, 7



;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "Ralink"
Ralink                      = "Ralink Technology Corp."
Amigo                       = "Amigo Technology Inc."
MSI                         = "802.11 Wireless"
SMC                         = "SMC Networks, Inc"

RALINK.DeviceDesc           = "RT2500 USB Wireless LAN Card"
AMIGO.DeviceDesc            = "802.11 g Wireless LAN Pocket USB"
m2500usb_6861.DeviceDesc    = "Wireless 11g USB 2.0 Stick"
m2500usb_6865.DeviceDesc    = "Wireless 11g MiniUSB 2.0 Adapter"
m2500usb_6869.DeviceDesc    = "Wireless 11g MiniUSB 2.0 Bluetooth Combo"
SMC.DeviceDesc              = "SMC Wireless USB Adapter"

INSTALL_DISK_STR            = "Wireless 11g USB Installation Disk"

RALINK.Service.DispName     = "RT2500 USB Wireless LAN Driver"
AMIGO.Service.DispName      = "RT2572 Wireless Driver"
m2500usb.Service.DispName   = "Wireless 11g USB 2.0 Network Driver"
SMC.Service.DispName        = "SMC USB Wireless LAN Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = ""
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
